Sensors - Graphic - Actuators - Sensors Configuration - System Configuration - Help
Help
AVR®32 UC3 Control Panel

## Control Panel Source

The control Panel is part of the AVR32 UC3 Software Framework. For more information, refer to the Control Panel User's Guide: /APPLICATIONS/EVK1100-CONTROL-PANEL/readme.html

## Control Panel Features

### 1. ADC data acquisition

From sensors and actuators as logs. These logs are saved in text files on the embedded file system FAT on the EVK1100's dataflash.

### 2. An embedded web server

Allowing a remote user to consult the logs and set the actuators in real time and configure the Control Panel modules through any web browser.

### 3. A USB Mass Storage device

Allowing a USB host to connect to the board and browse the Control Panel embedded file system. As mentionned on the LCD on line 3 "Press -> Mass Storage", press the joystick to switch to Mass Storage device mode. You may now plug a USB host to the EVK1100 board to enter the USB device mass storage mode (note that the message on the LCD on line 3 has changed to "Waiting for Host" then to "USB Mass Storage").

### 4. A USB Mass Storage host

Allowing to plug a Mass Storage USB key onto the board. The Control Panel then acts as a USB host and the user may actions using the local man-machine interface. Plug your USB key to a miniA plug to STD-A Receptacle OTG cable to adapt to the miniA-B receptacle on the board the Control Panel is running on. Then plug the cable to the board. You shall see the USB sign appear on the LCD(last column of the second line). The symbol on the last column of the menu line(a right arrow) tells the user that there is new actions in this menu to perform.

### 5. A Shell-like interface

On the EVK1100 USART_0 (57600bps/8bit data/1 stop bit/no flow control), allowing to navigate on the Control Panel file system, to configure the system, to interface with the sensors and actuators.

### 6. A RS-232 debug output

On the EVK1100 USART_1 (57600bps/8bit data/1 stop bit/no flow control).