/* ------------------------------------------------------------------------------------------------ */
/* FILE :        Platform.txt																		*/
/*																									*/
/* CONTENTS :																						*/
/*               Explanation for the platform numbering and list of supported platform				*/
/*																									*/
/*																									*/
/* Copyright (c) 2016-2018, Code-Time Technologies Inc. All rights reserved.						*/
/*																									*/
/* Code-Time Technologies retains all right, title, and interest in and to this work				*/
/*																									*/
/* THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS							*/
/* OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF										*/
/* MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT SHALL							*/
/* THE AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR								*/
/* OTHER LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE,							*/
/* ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR							*/
/* OTHER DEALINGS IN THE SOFTWARE.																	*/
/*																									*/
/*																									*/
/*	$Revision: 1.7 $																				*/
/*	$Date: 2018/01/09 22:14:53 $																	*/
/*																									*/
/* ------------------------------------------------------------------------------------------------ */

	Abassi (mainly assembly code) and the Demos use a number to identify the target platform.

	For Abassi, the platform number is only used to be informed of the target device.
	For the demos, this is mainly to inform the demo code what is the target board, in order to
	know how to access the LEDs, buttons, I2C, Ethernet etc.

	The board & device are defined through the build option OS_PLATFORM and is always a hex number.
	The last 6 nibbles define a unique device or device family and the upper 2 nibbles define the
    board for that device. Each device family have a unique group of 2,3 or 4 nibbles to identify
    them.  The unique set of nibbles is shown in parentheses, e.g for i.MX6 (0x....FEE6).

	If the demos are re-used for you custom board, it would be a good idea to number your custom
	board at 0xFF000000, as this value would most likely never be used by Code Time demos.
	For example, assuming your target device is an Arria 10, then you should use 0xFF00AA10 as
	the value for OS_PLATFORM.  The 4 lower nibbles (0xAA10) uniquely identifies the Arria 10 and
	your custom board for the Arria 10 is #0xFF.

	All target dependent defintions are loacted in these 2 files:
			Platform.h
			HWinfo.h
	Platform.h contains all the information related ot the processor itself
	           The defintions are grouped in two sections.
	           1st - the processor itself, irrelevent of the clock, or what is connected to it.
	                 defines the interrupt #, DMA channels etc
	           2nd - outside of the processor, irrelevent of the peripherals
	                 defines the clock and which devices are connected. e.g. UART device #
	HWinfo.h contains all the information related to the peripherals on the target platform
	           e.g. number of switches & LEDs and how to access them

/* ------------------------------------------------------------------------------------------------ */

ARM Cortex A9

	Cyclone V  (0x..00AAC5)
                0x0000AAC5		Cyclone V SocFPGA development board
                0x0100AAC5		DE0-Nano / DE10-nano / Atlas evaluation board
                0x0200AAC5		EBV Socrates evaluation board
	Arria V    (0x..00AAC5)		(note: same dev # as Cyclone V because HPSs are the same)
                0x4000AAC5		Arria V SocFPGA development board
	Arria 10   (0x..00AA10)
                0x0000AA10		Arria 10 SocFPGA development board
	i.MX6      (0x..00FEE6)
                0x0000FEE6		i.MX6 Sabrelite evaluation board
	OMAP	   (0x..0044..)
                0x00004460		Panda board with OMAP 4460
	Zynq 7020  (0x..007020)
                0x00007020		Zynq 7020 Zedboard

/* ------------------------------------------------------------------------------------------------ */

ARM Cortex A9

	UltraScale+ (0x..007753)
                 0x00007753		A53s on the ZCU-102

/* ------------------------------------------------------------------------------------------------ */

ARM Cortex M0

	LPCXXXXXX: (0x..0C....)
				0x000C1124		NGX Technologies BlueBoard LPC11U24 evaluation board
				0x000C1227		Olimex LPC1227-STK evaluation board

/* ------------------------------------------------------------------------------------------------ */

ARM Cortex M3

	LM3SXXXX:  (0x..35....)
				0x00351968		TI's EKLM3S1968 evaluation board
	LPCXXXXXX: (0x..3C....)
				0x003C1343		NGX Technologies BlueBoard LPC1343 evaluation board
				0x003C1766
	STM32F1XX: (0x..32F1..)
				0x1032F107		Olimex STM32-P107 board (STM32F107)
	STM32F2XX: (0x..32F2..)
				0x0032F207		STM3220G development board (STM32F207)
				0x1032F207		Olimex STM32-P207 board (STM32F207)

/* ------------------------------------------------------------------------------------------------ */

ARM Cortex M4

	STM32F4XX: (0x..32F4..)
				0x0032F407		STM32F4 Discovery board (STM32F407)
				0x1032F407		Olimex STM32-P407 board (STM32F407)

/* ------------------------------------------------------------------------------------------------ */

ARM Cortex R5

	UltraScale+	(0x..007705)
                 0x00007705		R5s on the ZCU-102

/* ------------------------------------------------------------------------------------------------ */

AVR

	ATmega:    (0x..AE8...
				0x00AE8128		Olimex AVR-MT-128 evaluation board

/* ------------------------------------------------------------------------------------------------ */

AVR32A

	UC3B:      (0x..AEA...)
				0x00AEA101		Atmel EVK1101 evaluation board

/* ------------------------------------------------------------------------------------------------ */

ColdFire       (0x..CF....)
				0x00CF5223		Freescale M52233DEMO evaluation board	

/* ------------------------------------------------------------------------------------------------ */

C28X

	P28X:      (0x..028...)
				0x00028027		Olimex TMX320-P28027 evaluation board 

/* ------------------------------------------------------------------------------------------------ */

MSP430

	MSP430:    (0x..43....)
				0x00431611		Olimex MSP430-P1611 evaluation board
	MSP430X:   (0x..44....)
				0x00445438		Olimex MSP-5438STK evaluation board

/* ------------------------------------------------------------------------------------------------ */

PIC32          (0x..320...)
				0x00320000		Olimex PIC32-WEB evaluation board

/* ------------------------------------------------------------------------------------------------ */

8051

	Generic:   (0x..008051)
				0x00008051		Standard 8051 device

/* ------------------------------------------------------------------------------------------------ */

80251

	Generic:   (0x..080251)
				0x00080251		Standard 80251 device

/* ------------------------------------------------------------------------------------------------ */

/* EOF */
